CISCO

Equipos

SF300

Default

Usuario	cisco
Password	cisco

Comandos

boot	Boot Commands
clear	Reset functions
clock	Manage the system clock
configure	Enter configuration mode
copy	Copy from one file to another
crypto	Cryptographic commands
debug-mode	Exit from the EXEC to debug mode
delete	Delete a file from the flash file system
dir	Display the list of files on the flash file system
disable	Disable privileged commands
dot1x	802.1x EXEC commands
exit	Exit from the EXEC
green-ethernet	Green ethernet commands
help	Description of the interactive help system
ip	Global IP configuration commands
login	Exit from the EXEC and Log in
macro	Ports macros
menu	Enter into Menu-CLI
more	Display a file
no	Negate command
ping	Send echo messages.
reload	Halt and perform a cold restart
rename	Rename a file
renew	Renew DHCP address
resume	Resume telnet session.
set	Set System Parameters
show	Show running system information
telnet	Open telnet session.
terminal	Set current session functions
test	diagnose
traceroute	Discover the routes to destination.
write	Write running configuration to memory or terminal

Habilitar SSH

switchf63292#configure terminal
switchf63292(config)#ip ssh server
switchf63292(config)#end
switchf63292#

Configuración Minicom

pu port /dev/ttyUSB0 pu baudrate 115200 pu xonxoff No pu bits 8 pu parity N pu stopbits 1 pu hasdcd No pu rtscts No